|  |
| --- |
| ***REPLACE WITH YOUR MASTHEAD*** |
| **VFIS logo black JPG** | **SOG Title:** |
| **SOG Number:** |
| **Original Date:** | **Revision Date:** |
| **ABC Fire Department General Operating Guideline** |

**Stopped School Bus**

***This is a sample of a standard operating guideline (SOG) on this topic. You should review the content, modify as appropriate for your organization, have it reviewed by your leadership team and if appropriate your legal counsel. Once adopted, make sure the SOG is communicated to members, implemented and performance monitored for effective implementation.***

**Purpose:**

To establish safe practices that address when an emergency vehicle comes to a school bus that has stopped with red lights flashing.

**Procedure:**

The emergency vehicle **shall not pass a school bus that has stopped with red lights flashing** to load or discharge passengers, unless the bus driver clearly signals that it is safe to pass.

When clearly signaled by the bus driver that it is safe to pass a stopped school bus, the emergency vehicle shall proceed slowly and with extreme caution past the school bus; all members must be vigilant for children while approaching and passing the bus. The emergency vehicle driver must be prepared to stop immediately while approaching, passing, and leaving the area in which the school bus is stopped.

***This is a sample guideline furnished to you by VFIS. Your organization should review this guideline and make the necessary modifications to meet your organization’s needs. The intent of this guideline is to assist you in reducing exposure to the risk of injury, harm or damage to personnel, property and the general public. For additional information on this topic, contact your VFIS Risk Control representative.***

**References:**

West Redding (CT) VFD – GOG 10-EVO-1019 Developed/Revised/Reviewed by VFIS ETC